|  |  |
| --- | --- |
| **Steps to Build**  **WFWC Wool Tromping Stand**  Please refer to schematic and images on website | C:\Users\Eileen\Pictures\5392845_orig.jpg |

|  |  |
| --- | --- |
|  |  |
|  |  |
| **Step 1** | Weld each of 4 Sections. Each Section is 4 lengths of angle iron. |
|  |  |
| **Step 2** | Clamp all 4 Sections together to form a square. When square,  tack-weld the stand in several places. This ensures stability. |
|  |  |
| **Step 3** | Weld on the Hinges and the Locking Pin Sleeves. |
|  |  |
| **Step 4** | Remove tack-welds. |
|  |  |
| **Step 5** | Weld on each of the 5 Wheels. |
|  |  |
| **Step 6a** | Weld Locking Pins to Locking Pin Chains. |
|  |  |
| **Step 6b** | Weld each Locking Pin Chain assembly to Stand. |
|  |  |
| **Step 6c** | Weld on Gate Locking Rivets. |
|  |  |
| **Step 7a** | Weld on Nail Backing Plates. |
|  |  |
| **Step 7b** | Drill Nail Holes. The Holes must be vertical. |
|  |  |
| **Step 8** | Paint Stand to avoid rust. |
|  |  |
|  | **Optional** |
|  |  |
| **Step 1a** | Add a Step. Weld 1 horizontal length of angle iron 16” up from the bottom length. |
|  |  |
| **Step 5a** | Add an Armrest. Weld 3 lengths of angle iron to 1 Section of the Stand. |